Cisco Internetwork Operating System Software 
IOS (tm) C2900XL Software (C2900XL-H2-M), Version 12.0(5.1)XP, MAINTENANCE INTERIM SOFTWARE
Copyright (c) 1986-1999 by cisco Systems, Inc.
Compiled Fri 10-Dec-99 11:00 by cchang
Image text-base: 0x00003000, data-base: 0x00282880

ROM: Bootstrap program is C2900XL boot loader

Switch uptime is 43 minutes
System returned to ROM by power-on
System image file is "flash:c2900XL-h2-mz-120.5.1-XP.bin"


cisco WS-C2924-XL (PowerPC403GA) processor (revision 0x11) with 8192K/1024K bytes of memory.
Processor board ID 0x0E, with hardware revision 0x01
Last reset from power-on

Processor is running Standard Edition Software
Cluster member switch capable
24 FastEthernet/IEEE 802.3 interface(s)

32K bytes of flash-simulated non-volatile configuration memory.
Base ethernet MAC Address: 00:01:42:98:7D:40
Motherboard assembly number: 73-3382-07
Power supply part number: 34-0834-01
Motherboard serial number: FAB040741B2
Power supply serial number: DAB03504K5D
Model revision number: A0
Motherboard revision number: E0
Model number: WS-C2924-XL-A
System serial number: FAB0408T0EQ
Configuration register is 0xF