Cisco Internetwork Operating System Software 
IOS (tm) 2500 Software (C2500-JS-L), Version 12.0(9), RELEASE SOFTWARE (fc1)
Copyright (c) 1986-2000 by cisco Systems, Inc.
Compiled Mon 24-Jan-00 22:30 by bettyl
Image text-base: 0x03051D64, data-base: 0x00001000

ROM: System Bootstrap, Version 5.2(8a), RELEASE SOFTWARE
BOOTFLASH: 3000 Bootstrap Software (IGS-RXBOOT), Version 10.2(8a), RELEASE SOFTWARE (fc1)

ROUTER2 uptime is 2 hours, 14 minutes
System restarted by power-on
System image file is "flash:c2500-js-l_120-9.bin"

cisco 2500 (68030) processor (revision B) with 16384K/2048K bytes of memory.
Processor board ID 01413911, with hardware revision 00000000
Bridging software.
X.25 software, Version 3.0.0.
SuperLAT software (copyright 1990 by Meridian Technology Corp).
TN3270 Emulation software.
1 Token Ring/IEEE 802.5 interface(s)
2 Serial network interface(s)
32K bytes of non-volatile configuration memory.
16384K bytes of processor board System flash (Read ONLY)
          
Configuration register is 0x2102