Cisco Internetwork Operating System Software 
IOS (tm) 3600 Software (C3640-JS-M), Version 12.0(9), RELEASE SOFTWARE (fc1)
Copyright (c) 1986-2000 by cisco Systems, Inc.
Compiled Wed 26-Jan-00 18:38 by bettyl
Image text-base: 0x60008918, data-base: 0x60C04000

ROM: System Bootstrap, Version 11.1(20)AA2, EARLY DEPLOYMENT RELEASE SOFTWARE (fc1)

Router uptime is 2 hours, 22 minutes
System restarted by power-on
System image file is "flash:c3640.bin"

cisco 3640 (R4700) processor (revision 0x00) with 59392K/6144K bytes of memory.
Processor board ID 15888885
R4700 processor, Implementation 33, Revision 1.0
Bridging software.
X.25 software, Version 3.0.0.
SuperLAT software (copyright 1990 by Meridian Technology Corp).
TN3270 Emulation software.
1 Ethernet/IEEE 802.3 interface(s)
1 FastEthernet/IEEE 802.3 interface(s)
1 Token Ring/IEEE 802.5 interface(s)
1 Serial network interface(s)
2 Voice FXO interface(s)
2 Voice FXS interface(s)
DRAM configuration is 64 bits wide with parity disabled.
125K bytes of non-volatile configuration memory.
16384K bytes of processor board System flash (Read/Write)

Configuration register is 0x2102