Cisco Internetwork Operating System Software 
IOS (tm) LS1010 W5-9 Software (LS1010-WP-M), Version 12.0(3c)W5(9),  RELEASE SOFTWARE 
Copyright (c) 1986-1999 by cisco Systems, Inc.
Compiled Mon 10-May-99 19:03 by integ
Image text-base: 0x60010930, data-base: 0x60756000

ROM: System Bootstrap, Version 11.2(1.4.WA3.0) [integ 1.4.WA3.0], RELEASE SOFTWARE

Switch uptime is 2 minutes
System restarted by power-on
System image file is "bootflash:ios.Z"

cisco LS1015 (R4600) processor with 65536K bytes of memory.
R4700 processor, Implementation 33, Revision 1.0
Last reset from power-on
1 Ethernet/IEEE 802.3 interface(s)
5 ATM network interface(s)
123K bytes of non-volatile configuration memory.

8192K bytes of Flash internal SIMM (Sector size 256K).
Configuration register is 0x2101


Slot Ctrlr-Type      Part No.  Rev  Ser No  Mfg Date   RMA No. Hw Vrs  Tst EEP
---- --------------  ---------- -- -------- --------- -------- ------- --- ---
12/0  155MM PAM       73-1496-04 A0 15353529 May 18 00 00-00-00   4.0     0   2
13/0  ATM Swi/Proc    68-0732-01 C0 14340650 Jul 20 99 00-00-00   6.0     0   2
13/1  FC-PFQ          73-2281-04 B0 14341271 Jul 20 99 00-00-00   4.2     0   2

DS1201 Backplane EEPROM:
Model Ver.  Serial  MAC-Address  MAC-Size  RMA  RMA-Number   MFG-Date
----- ---- -------- ------------ --------  ---  ----------  -----------
ws-C5500  2   69047857 0050A2C76800   1024      0        0      Oct 17 1998

