Cisco Internetwork Operating System Software 
IOS (tm) 2500 Software (C2500-JS-L), Version 12.0(9), RELEASE SOFTWARE (fc1)
Copyright (c) 1986-2000 by cisco Systems, Inc.
Compiled Mon 24-Jan-00 22:30 by bettyl
Image text-base: 0x03051D64, data-base: 0x00001000

ROM: System Bootstrap, Version 11.0(10c), SOFTWARE
BOOTFLASH: 3000 Bootstrap Software (IGS-BOOT-R), Version 11.0(10c), RELEASE SOFTWARE (fc1)

ROUTER4 uptime is 2 hours, 17 minutes
System restarted by power-on
System image file is "flash:c2500-js-l_120-9.bin"

cisco 2500 (68030) processor (revision N) with 14336K/2048K bytes of memory.
Processor board ID 08858014, with hardware revision 00000001
Bridging software.
X.25 software, Version 3.0.0.
SuperLAT software (copyright 1990 by Meridian Technology Corp).
TN3270 Emulation software.
Basic Rate ISDN software, Version 1.1.
1 Ethernet/IEEE 802.3 interface(s)
2 Serial network interface(s)
1 ISDN Basic Rate interface(s)
32K bytes of non-volatile configuration memory.
16384K bytes of processor board System flash (Read ONLY)

Configuration register is 0x2102