Cisco Internetwork Operating System Software 
IOS (tm) 2500 Software (C2500-JS-L), Version 12.0(9), RELEASE SOFTWARE (fc1)
Copyright (c) 1986-2000 by cisco Systems, Inc.
Compiled Mon 24-Jan-00 22:30 by bettyl
Image text-base: 0x03051D64, data-base: 0x00001000

ROM: System Bootstrap, Version 5.2(8a), RELEASE SOFTWARE
BOOTFLASH: 3000 Bootstrap Software (IGS-RXBOOT), Version 10.2(8a), RELEASE SOFTWARE (fc1)

ROUTER1 uptime is 2 hours, 12 minutes
System restarted by power-on
System image file is "flash:c2500-js-l_120-9.bin"

cisco 2500 (68030) processor (revision L) with 14336K/2048K bytes of memory.
Processor board ID 01504261, with hardware revision 00000000
Bridging software.
X.25 software, Version 3.0.0.
SuperLAT software (copyright 1990 by Meridian Technology Corp).
TN3270 Emulation software.
Basic Rate ISDN software, Version 1.1.
1 Token Ring/IEEE 802.5 interface(s)
2 Serial network interface(s)
1 ISDN Basic Rate interface(s)
32K bytes of non-volatile configuration memory.
16384K bytes of processor board System flash (Read ONLY)
          
Configuration register is 0x2102